[Information]
; (Latest Translator, First Translator, Second Translator ...)
TRANSLATOR=Alexei PortableApp™, Jan Verheijen, Albert CLAESEN, Luc, Adrien Brysse
VERSION=7.2.0

[Language]
LANGUAGE=Nederlands
CHARACTER_CODE=Unicode (UTF-16, LE, w/ BOM)
LOCALE_ID=0x0413, 0x0813

[Url]
WIKIPEDIA_SMART=https://de.wikipedia.org/wiki/Self-Monitoring%2C_Analysis_and_Reporting_Technology

[Menu]
FILE=&Bestand
CUSTOMIZE=&Aanpassen
EXIT=&Afsluiten
EDIT=&Bewerken
COPY=&Kopiëren
FUNCTION=F&uncties
HIDE_SMART_INFO=&S.M.A.R.T.-informatie verbergen
HIDE_SERIAL_NUMBER=Serie&nummer verbergen
SHOW_DRIVE_LETTER=Schijf&letter weergeven
ADVANCED_DISK_SEARCH=G&avanceerd Schijfzoeken
EVENT_LOG=&Gebeurtenis Logboek
AAM_APM_CONTROL=AA&M/APM-beheer
AUTO_AAM_APM_ADAPTION=Auto-AAM/A&PM-aanpassen
RESIDENT=Toon In Systeemvak (Afsluiten d.m.v. RechtermuisMenu op Pict!)
STARTUP=Met Windows Starten (n.v.t. Portable)
OPEN_DISK_MANAGEMENT=&Schijfbeheer openen
OPEN_DEVICE_MANAGER=Apparaatbeheer openen
ADVANCED_FEATURE=Geavanceerde-Functies
REFRESH=&Vernieuwen
RESCAN=Her-Scannen
DISABLE=&Uitschakelen
AUTO_REFRESH=&Auto-vernieuwen interval
AUTO_REFRESH_TARGET=Auto-vernieuwen object
AUTO_REFRESH_TARGET_ALL_DISK=Auto-vernieuwen - Alle schijven
AUTO_REFRESH_UNTARGET_ALL_DISK=Auto-vernieuwen - Geen schijven
WAIT_TIME_AT_STARTUP=&Wachttijd bij opstarten
GRAPH=&Grafiek
THEME=&Thema
DISK=&Schijf
HELP=&Help
HELP_WEB=&Help [Web]
HELP_ABOUT=&Over CrystalDiskInfo
HELP_ABOUT_SMART=Over &S.M.A.R.T. (Wikipedia) [Web]
LANGUAGE=Taal 
ITEM=&Item
TEMPERATURE_TYPE=T&emperatuur Type
CELSIUS=Celsius (°C)
FAHRENHEIT=Fahrenheit (°F)
HEALTH_STATUS_SETTING=&Gezondheid Status Instelling

;Graph
OPTION=&Optie
LEGEND_POSITION=&Legenda Positie
NORTH_WEST=&Noord-West
NORTH_EAST=Noord-&Oost
SOUTH_WEST=Zuid-&West
SOUTH_EAST=&Zuid-Oost
MAX_PLOT_POINT=&Max plotpunten
TIME_FORMAT=&Tijdformaat
PAINT_WEEKEND=Weekend kleuren
ALL=&Alles

;2.7.0
COPY_OPTION=Kopieer& Optie
RESIDENT_STYLE=Taakvak st&ijl
MINIMIZE=Minimaliseren
HIDE=Verbergen

;3.0.0
ZOOM=&Zoomen
AUTO=&Auto
ATTRIBUTE=&Kenmerk

;3.5.0
ASCII_VIEW=ASCII-Weergave
AUTO_DTECTION=Auto Detectie
SECOND=Sec.
MINUTE=Min.
HOUR=Uur

:3.9.4
WORKAROUND=Werkomgeving

;4.0.0
ALERT_MAIL=Waarschuwing-Mail
MAIL_SETTINGS=Mail-Instellingen
SMART_IN_ENGLISH=S.M.A.R.T. in het Engels
FONT_SETTING=Lettertype-Instelling

;5.0.0
ALERT_FEATURES=Waarschuwing-Functies
ALARM_HISTORY=Alarm Geschiedenis
ALERT_SOUND=Waarschuwing-Geluid
SOUND_SETTINGS=Geluid Instellingen
GADGET_SUPPORT=Gadget-Ondersteuning
INSTALL_GADGET=Gadget Installeren
ENABLE_AUTO=Inschakelen (Autodetectie)
ENABLE_ALL=Inschakelen (Alle schijven)
ENABLE_RAID=Inschakelen (Alleen RAID)

;6.0.0
HIDE_NO_SMART_DISK=&Verberg Non-S.M.A.R.T. Schijf
GREEN_MODE=&Groene Modus

;8.6.0
SAVE_TEXT=Save (&text)
SAVE_IMAGE=&Save (image)

;9.0.0
DRIVE_SORT_METHOD=Drive Sort Method
PHYSICAL_DRIVE_ID=Physical Drive ID
DRIVE_LETTER=Drive Letter

;9.2.0
VOICE=Voice

[TrayMenu]
EXIT=Afsluiten
REFRESH=Vernieuwen
RESCAN=Her-Scannen
ENABLE=Inschakelen
DISABLE=Uitschakelen
ENABLE_ALL=Alles inschakelen
DISABLE_ALL=Alles uitschakelen
AUTO_REFRESH=Auto-vernieuwen
AUTO_REFRESH_01_MIN=1 min.
AUTO_REFRESH_03_MIN=3 min.
AUTO_REFRESH_05_MIN=5 min.
AUTO_REFRESH_10_MIN=10 min.
AUTO_REFRESH_30_MIN=30 min.
AUTO_REFRESH_60_MIN=60 min.
AUTO_REFRESH_TARGET=Auto-vernieuwen object
AUTO_REFRESH_TARGET_ALL_DISK=Auto-vernieuwen -  Alle schijven
AUTO_REFRESH_UNTARGET_ALL_DISK=Auto-vernieuwen - Geen schijven
ALARM_SETTING_TEMPERATURE=Alarminstelling - Temperatuur
ALARM_SETTING_HEALTH_STATUS=Alarminstelling - Gezondheid Status
SHOW_MAIN_WINDOW=Hoofdvenster weergeven
SHOW_TEMPERATURE_ICON=Temperatuur Pictogram weergeven
SHOW_ALL_TEMPERATURE_ICON=Alle Temperatuur Pictogrammen weergeven
HIDE_ALL_TEMPERATURE_ICON=Alle Temperatuur Pictogrammen verbergen
COLLECTIVE_SETTING=Gemeenschappelijke instelling
GRAPH=Grafiek
;Added 3.0
SHOW_TEMPERATURE_ICON_ONLY=Alleen Temperatuur Pictogram weergeven

[DiskStatus]
GOOD=Goed
CAUTION=Waarschuwing
BAD=Slecht
UNKNOWN=Onbekend
DISK=Schijf

[Dialog]
LIST_ID=ID
LIST_CURRENT=Huidig
LIST_WORST=Slechtste
LIST_THRESHOLD=Drempel
LIST_RAW_VALUES=Raw-Waarden
LIST_DESCRIPTION=Omschrijving
LIST_ATTRIBUTE_NAME=Kenmerk

FIRMWARE=Firmware
SERIAL_NUMBER=Serienummer
INTERFACE=Interface
STANDARD=Standaard
TRANSFER_MODE=Transfer-Modus
BUFFER_SIZE=Buffer Grootte
NV_CACHE_SIZE=NV-Cache Grootte
ROTATION_RATE=Rotatie Per Minuut
TEMPERATURE=Temperatuur
POWER_ON_HOURS=Bedrijfs Uren
POWER_ON_COUNT=Inschakelingen
DRIVE_LETTER=Schijfletter
FEATURE=Eigenschappen
HEALTH_STATUS=Gezondheid Status

UNKNOWN=onbekend
POWER_ON_COUNT_UNIT=keer
POWER_ON_HOURS_UNIT=uren
POWER_ON_DAYS_UNIT=dagen
POWER_ON_YEARS_UNIT=jaar

;4.3
TOTAL_HOST_WRITES=Schrijf Acties Totaal
TOTAL_HOST_READS=Lees Acties Totaal
TOTAL_NAND_WRITES=NAND-Schrijf Acties

;4.5
WEAR_LEVELING_COUNT=Slijtage Niveau

;6.1
CURRENT_MODE_SUPPORTED_MODE=Huidige Modus | Ondersteunde Modus
MAJOR_VERSION_MINOR_VERSION=Hoofd Versie | Sub Versie

;8.5.0
FONT_FACE=Font Face
FONT_SCALE=Font Scale (%)
DEFAULT=Default

;8.9.0
ENABLED=Enabled
DISABLED=Disabled

[Message]
DETECT_UNIT_POWER_ON_HOURS=Bepalen van bedrijfsuren (ca. 130 sec. nodig)
DETECT_DISK=Schijf detecteren
PLEASE_ENABLE_WMI=WMI(Windows Management Instrumentation) inschakelen
PLEASE_RESTART_THIS_APPLICATION=Herstart dit programma a.u.b., om de wijzigingen door te voeren
DISK_NOT_FOUND=Schijf niet gevonden

[Alarm]
ALARM_TEMPERATURE=Temperatuur - Alarm
ALARM_HEALTH_STATUS=Gezondheid Status - Alarm
DEGRADATION=Degradatie
RECOVERY=Herstellen
;3.5.0
INFO_HEALTH_STATUS=Info - Gezondheid Satus

[Graph]
PLEASE_SELECT_ITEM=Een item selecteren a.u.b.
ACTUAL_VALUE=Huidige waarde (Raw-waarde)
NORMALIZED_VALUE=Genormaliseerde waarde (huidige waarde)
ALL_ON=Alles aan
ALL_OFF=Alles uit
RESET=Terugzetten

[Customize]
LINE_COLOR=Lijnkleur
BACKGROUND_IMAGE=Achtergrond Afbeelding
SUPPORTED_IMAGE_FORMAT=Ondersteund Afbeelding Formaat
ALL_FILES=Alle bestanden

;5.0.0
SUPPORTED_SOUND_FORMAT=Ondersteunde Geluids Formaat

[AamApm]
AAM_LOW=<- Stil (80h)
AAM_HIGH=Prestatie (FEh) ->
AAM_RECOMMEND=Aanbevolen waarde
APM_LOW=<- Min Vermogen (01h)
APM_HIGH=Prestatie (FEh) ->
;3.5.0
AUTOMATIC_ACOUSTIC_MANAGEMENT=Automatisch Acoustisch Management (AAM)
ADVANCED_POWER_MANAGEMENT=Geavanceerd Power Management (APM)

[WindowTitle]
ABOUT=Over CrystalDiskInfo
GRAPH=Grafisch
CUSTOMIZE=Aanpassen
VERSION_INFORMATION=Versie-Informatie
AAM_APM_CONTROL=AAM/APM-beheer
HEALTH_STATUS_SETTING=Gezondheid Status Instelling

;5.0.0
ALARM_HISTORY=Alarm Geschiedenis
SOUND_SETTINGS=Geluids Instellingen

;5.1.0
FONT_SETTING=Lettertype-Instelling

[HealthStatus]
THRESHOLD_OF_CAUTION=Waarschuwingsgrens
APPLY=Toepassen
DEFAULT=Standaard

[Smart]
UNKNOWN=Onbekend
VENDOR_SPECIFIC=Concrete Leverancier
01=Lees Fout Factor
02=Data Doorvoersnelheid
03=Opstart Tijd
04=Start/Stop Aantal
05=Heringedeelde Sectoren
06=Lees Kanaal Marge
07=Zoek Fouten Factor
08=Zoek tijd prestaties
09=Bedrijfs Uren
0A=Herstart's
0B=Herijkingen
0C=Power Cyclus
0D=Soft Lees Fout Factor stab
B8=End-to-End Fout
BB=Gerapporteerde Niet Corrigeerbare Fouten
BC=Opdracht Timeout
BD=High Fly Schrijft
BE=Luchtstroom Temperatuur
BF=G-Sensor Fout Factor
C0=Power-Uit Intrekken
C1=Laden/Ontladen Cyclus
C2=Temperatuur
C3=Hardware ECC Hersteld
C4=Heringedeelde Events
C5=Huidig Wachtende Sectoren
C6=Niet Corrigeerbare Sectoren
C7=UltraDMA CRC Fouten
C8=Schrijf Fout Factor
C9=Soft Lees Fout Factor
CA=Data Adres Markeer Fout
CB=Run Uit Annuleren
CC=Soft ECC Correctie
CD=Warmte Asperity Factor
CE=Flying Hoogte
CF=Huidig Spin Hoogte
D0=Draai Geluid
D1=Offline Zoek Prestatie
D3=Trilling Tijdens Schrijven
D4=Schokken tijdens schrijven
DC=Schijf Verschuiving
DD=G-Sensor Fout Factor
DE=Laad Uren
DF=Laden /Ontladen Opnieuw Testen
E0=Laad Wrijving
E1=Laden/Ontladen Cyclus
E2=Laad 'In'-Tijd
E3=Draaimomend Versterk Instelling
E4=Uitschakel Cyclus
E6=GMR Koppen Amplitude
E7=Temperatuur
F0=Koppen Flying Uren
FA=Leesfout Opnieuw Factor
FE=Vrije Val Bescherming

;Updated 5.4.0
F1=Totaal Host Schrijven
F2=Totaal Host Lezen

[SmartSsd]
01=Lees Fout Factor
02=Data Doorvoersnelheid
03=Spin-Opstart tijd
04=Start/Stop Aantal
05=Toegewezen Sectoren
06=Leeskanaal Responsie limiet
07=Zoek Fouten
08=Goede Zoek Acties
09=Bedrijfsuren
0A=Num. Mislukte Spindel Opstart
0B=Num. Noodzakelijke Her-Kalibratie
0C=Num. Inrichting inschakelen
0D=Software Lezen Fout Percentage
C0=Onjuiste Uitschakeling
C2=Temperatuur
C4=Toewijzen Events
C5=Momenteel Zwevende Sectoren
C6=Niet Corrigeerbare Sectoren
F1=Host Schrijf Voortgang (tot.)
F2=Host Lees acties (tot.)
; CrystalDiskInfo Toewijzen
FF=Resterend Levenduur

;Updated 5.4.0
F1=Totaal Host Geschreven
F2=Totaal Host Gelezen

[SmartMtron]
BB=Totaal Wissen

[SmartIndilinx]
01=Lees Fout Factor
09=Bedrijfs Uren
0C=Schijf inschakelen
B8=Eerste Block Fouten
C3=Program Failure Block Count
C4=Wis Fouten
C5=Lees Fouten Block
C6=Gelezen Sectoren Totaal
C7=Schrijf Sectoren Totaal
C8=Lees Opdrachten Totaal
C9=Schrijf Opdrachten Totaal
CA=Fouten bits van Flash Totaal
CB=Gelezen Sectoren met Corrigeerbare Bit Fouten Totaal
CC=Volledige Identificatie van Defecte block
CD=Maximum Specificatie van PE-Aantal
CE=Minimum Wis Aantal
CF=Maximum Wis Aantal
D0=Gem. Wis Aantal
D1=Resterend Levenduur

[SmartJMicron60x]
09=Bedrijfs Uren
0C=Schijf inschakelen
C2=Temperatuur
E5=Systeem ID, Flash ID
E8=Firmware Versie Informatie
E9=ECC Foutieve registratie
EA=Gem. Wis Aantal, Max. Wis Aantal
EB=Aantal - Foutvrij Block, SysteemBlock

[SmartIntel]
03=Opstart Tijd
04=Start/Stop Aantal
05=Hertoegewezen Sector Aantal
09=Bedrijfs Uren
0C=Power Inschakelingen
C0=Niet veilige afsluitingen
E1=Host Verschrijvingen
E8=Beschikbaar Gereserveerde Ruimte
E9=Media Wearout Indicator
B8=End to End Fout Detectie

;Updated 4.1.0
AA=Beschikbare Gereserveerde Ruimte
AB=Programma Fouten
AC=Wis Fouten
BB=iet Corrigeerbare Fouten

;Updated 4.3.0
AE=Onverwacht Power Onderbreking
E2=Timed Workload Media Wear
E3=Timed Workload Host Read/Write Ratio
E4=Timed Workload Timer
F1=Totaal LBAs Geschreven
F2=Totaal LBAs Gelezen
F9=Totaal NAND Geschreven

;Updated 5.5.0
B7=ATA Terug Schakelen
BE=Temperatuur
C7=CRC Fouten

;Updated 5.6.1
AF=Vermogensverlies Bescherming Mislukt
C2=Temperatuur
C5=Zwevende Sectoren

;Added 6.6.0
EA=Warmte Status

[SmartSamsung]
05=Heringedeelde Sectoren
09=Bedrijfs Uren
0C=Schijf inschakelen
AF=Programma Fouten (Chip)
B0=Wis Fouten (Chip)
B1=Hoeveelheid Slijtage Nivellering
B2=Gebruikte Reserve Block's (Chip)
B3=Gebruikte Reserve Block's (Totaal)
B4=Ongebruikte Reserve Block's (Totaal)
B5=Programma Fouten (Totaal)
B6=Wis Fouten (Totaal)
B7=Werktijd Slechte Block's (Totaal)
BB=Niet Corrigeerbare Fouten
BE=Luchtstroom Temperatuur
C2=Temperatuur
C3=ECC Fout Factor
C6=Off-Line Niet Corrigeerbare Fouten
C7=CRC Fouten
C9=Super cap Status
CA=SSD Modus Status
EB=POR Herstellen
F1=Tot. LBA Geschreven
F2=Tot. LBA Gelezen

;Added 6.6
AA=ngebruikte Reserve Block's (Chip) 
AB=Programma Fouten (Chip)
AC=Wis Fouten (Chip)
AD=Slijtage Nivellering
AE=Onverwachte Power Onderbrekingen
B8=Fout Detectie
E9=Normaal gebruik van media

[SmartSandForce] ;Updated 3.7.0
01=Raw Lees Fout Factor
05=End-to-End Data Fouten Gecorrigeerd
09=Bedrijfs Uren
0C=Schijf inschakelen
0D=Soft Lees Fout Factor
64=Gigabytes Gewist
AA=Reserve Block's
AB=Programma Fouten
AC=Wis Fouten
AE=Onverwachte Power Onderbrekingen
B1=Slijtage Range Delta
B5=Programma Fouten
B6=Wis Fouten
B8=Geraporteerde I/O Fout Detectie Code Fouten
BB=Gerapporteerde Niet Corrigeerbare Fouten
C2=Temperatuur
C3=On-the-Fly ECC Niet Corrigeerbare Fouten
C4=Heringedeelde Events
C6=Niet Corrigeerbare Sectoren
C7=SATA R-Fouten (CRC) Fout
C9=Niet Corrigeerbare Soft Lees fout Factor
CC=Soft ECC Correctie Factor
E6=Levenduur Curve Status
E7=SSD Levensduur
E8=Beschikbare Gereserveerde Ruimte
EB=SuperCap Gezondheid
F1=Tijdsduur schrijven van Host
F2=Tijdsduur Lezen van Host

[SmartJMicron61x] ;Added 3.9.0
01=Lees Fout Factor
02=Data Doorvoersnelheid
03=Opstart Tijd
05=Heringedeelde Sectoren
07=Zoek Fout Factor
08=Zoek Tijd Snelheid
09=Bedrijfs Uren
0A=Herstart's
0C=Schijf inschakelen
A8=SATA PHY Fouten
AF=Slechte Cluster's Tabellen (ECC Fout telling)
C0=Onverwachte Power onderbrekingen
C2=Temperatuur
C5=Zwevende Setctoren
AA=Slecht Block
AD=Wissen

[SmartMicron] ;Added 4.0.0/ Updated 6.6.0
; RAIN = Redundant Array of Independent NAND
01=Raw Lees Fout Factor
05=Heringedeelde NAND Block's
09=Bedrijfs Uren
0C=Schijf inschakelen
0D=Soft Fout Factor's
0E=Apparaat Capaciteit (NAND)
0F=Gebruikers Capaciteit
10=Reserve Blocks Beschikbaar
11=Resterende Reserve Block's
64=Tot. Wis Aantal
AA=Gereserveerde Block's
AB=Programma Fouten Teller
AC=Wis Fouten
AD=Gemiddelde Block Wissen
AE=Onverwachte Power onderbrekingen
B4=Niet gebruikte NAND Blocks
B5=Onaangepaste Toegang Teller
B7=SATA Interface Terugschakelingen
B8=Fout Correcties
BB=Gerapporteerde Niet Corrigeerbare Fouten
BC=Opdracht TimeOut's
BD=Fabrieks Slechte Blocks
C2=Temperatuur
C3=Cumulatieve ECC Bit Correcties
C4=Herverdeling Acties
C5=Huidige In de Wacht staande Sectororen
C6=Smart Off-line Scan Niet Corrigeerbare Fouten
C7=Ultra DMA CRC Fout Factor
CA=Percentage Levensduur Gebruikt
CE=Schrijf Fout Factor
D2=Succesvolle RAIN Herstellingen Geteld
EA=Totaal Bytes Gelezen
F2=Bescherming Vooruitgang Schrijven
F3=ECC Bits Gecorrigeerd
F4=ECC Cumulatieve Drempel Gebeurtenissen
F5=Cumulatief Programma NAND Pagina's
F6=Totaal Host Sector Geschreven
F7=Host Programma Pagina's Geteld
F8=Achtergrond Programma Pagina's Geteld

[SmartMicronMU02] ;Updated 6.6.0
; RAIN = Redundant Array of Independent NAND
01=Raw Read Error Rate
05=Heringedeelde Sectoren
09=Bedrijfs Uren
0C=Schijf inschakelen
0D=Soft Error Rate
0E=Device Capacity (NAND)
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Blocks
64=Totaal Wissen
AA=Gereserveerde Block's
AB=Programma Fouten
AC=Wis Fouten
AD=Gemiddeld Block-Wissen
AE=Onverwachte Power Onderbrekingen
B4=Ongebruikte Reserve NAND Blocks
B7=SATA Interface Terug Schakelen
B8=Fout Correcties
BB=Gerapporteerde Niet Corrigeerbare Fouten
BC=Command Timeout Count
BD=Fabrieks Slechte Block's
C2=Temperatuur
C3=Cumulative ECC Bit Correction Count
C4=Reallocation Event Count
C5=Huidig Wachtende Sectoren
C6=Smart Off-line Scan Uncorrectable Error Count
C7=Ultra DMA CRC Error Rate
CA=Percent Lifetime Used
CE=Write Error Rate
D2=Successful RAIN Recovery Count
EA=Total Bytes Read
F3=ECC Bits Corrected
F4=ECC Cumulative Threshold Events
F5=Cumulative Program NAND Pages
F6=Total Host Sector Writes
F7=Host Program Page Count
F8=Background Program Page Count

; Updated 6.6.0
A0=Uncorrectable Sector Count
A1=Valid Spare Blocks
A3=Initial Invalid Blocks
94=Totaal SLC Wissen
95=Maximum SLC Wissen
96=Minimum SLC Wissen
97=Gemiddeld SLC Wissen
A4=Totaal TLC Wissen
A5=Maximum TLC Wissen
A6=Minimum TLC Wissen
A7=Gemiddeld TLC Wissen
A9=Percentage Lifetime Remaining
B5=Program Fail Count
B6=Wis Fouten
C0=Power-off Retract Count
E8=Available Reserved Space
F1=Total LBA Write
F2=Total LBA Read
F5=Total TLC Write Count
F6=Total SLC Write Count
F7=RAID Recovery Count

[SmartOcz] ;Added 4.5.0
01=Raw Read Error Rate
03=Opstart Tijd
04=Start Stop Count
05=Heringedeelde Sectoren
09=Bedrijfs Uren
0C=Schijf inschakelen
E8=Totaal Schrijf Sectoren
E9=Gebruik Resterend

; Added 6.6.0
64=Totaal Block's Wissen
A7=SSD Beveiliging Modus
A8=SATA PHY Fouten
A9=Slechte Block's
AD=Wissen
B8=Fabrieks Slechte Block's
C0=Onverwachte Power Onderbrekingen
CA=Totaal Gecorrigeerde Bits
CD=Max Rated PE Counts
CE=Minimum Wissen
CF=Maximum Wissen
D3=SATA Uncorrectable Error Count
D4=NAND Page Reads During Retry
D5=Simple Read Retry Attempts
D6=Adaptive Read Retry Attempts
DD=Internal Data Path Uncorrectable Errors
DE=RAID Herstellen
E6=Vermogensverlies Bescherming
FB=NAND Lezen

;Updated 6.7.0
F1=Totaal Host Schrijven
F2=Totaal Host Lezen

[SmartPlextor] ;Added 5.1.0
01=Lees Fout Factor
05=Heringedeelde Sectoren
09=Bedrijfs Uren
0C=Schijf inschakelen
C0=Onveilge Afsluitingen
C4=Reallocation Event Count
C6=Niet Corrigeerbare Sectoren
F1=Totaal Host Schrijven
F2=Totaal Host Lezen

;Updated 5.4.0
B1=Slijtage Egalisaties
B2=Gebruikte Gereserveerde Block's (slechtste geval)
B5=Program Fail Count
B6=Wis Fouten
BB=Niet Corrigeerbare Fouten
C7=Ultra CRC Fouten
E8=Beschikbare Gereserveerde Ruimte

;Added 6.2.0
AA=Groeiende Slechte Block's
AB=Programma Fouten
AC=Wis Fouten
AD=Gemiddeld Programma/Wissen
AE=Onverwachte Power Onderbrekingen
AF=Programma Fouten (Worst Case)
B0=Wis Fouten (Worst Case)
B3=Niet gebruikte Block's
B4=Ongebruikte Gereserveerde Block's (Totaal)
B7=SATA Interface Terug Geschakeld
B8=End-to-End Data Fouten Gecorrigeerd
BC=Opdracht Time out
C3=ECC Factor
E9=NAND GB Schrijven

[SmartSanDisk] ;Added 5.2.0
05=End-to-End Data Fouten Gecorrigeerd
09=Bedrijfs Uren
0C=Schijf inschakelen
AA=Reserve Block's
AB=Programma Fouten
AC=Wis Fouten
AE=Onverwachte Power Onderbrekingen
BB=Niet Corrigeerbare Fouten
E8=Levens Resterend
F1=Totaal Host Geschreven
F2=Totaal Host Gelezen

[SmartOczVector] ;Added 5.3.0
05=Verzamelde Werktijd Slechte Block's
09=Bedrijfs Uren
0C=Schijf inschakelen
AB=Beschikbare Over-Provisioned Block's
AE=Power Cycle (Niet Gepland)
BB=Totaal Niet Corrigeerbare NAND Gelezen
C3=Totaal Programering Fouten
C4=Totaal Wis Fouten
C5=Totaal Lees Fouten (Niet Corrigeerbare)
C6=Host Gelezen
C7=Host Geschreven
D0=Gemiddeld Gewist
D2=SATA CRC Fouten
E9=Levensduur Resterend
F9=NAND Programering

;Updated 5.5.0
F1=Totaal Host Geschreven
F2=Totaal Host Gelezen

;Updated 6.6.0
64=Totaal Block's Gewist
B8=Totaal Fabrieks Slechte Block's
CA=Totaal Gelezen Bits Gecorrigeerd
CD=Max. Factoren PE
CE=Min. Gewist
CF=Max. Gewist
D4=Totaal NAND Pagina's lezen die nodig hebben om opnieuw te lezen
D5=Totaal nieuwe eenvoudige lees pogingen
D6=Totaal of Adaptive Read Retry Attempts
DD=Intern Data Pad bescherming Niet Corrigeerbare Fouten
DE=RAID Herstel
E0=In Garantie
E1=DAS Polariteit
E2=Gedeeltelijke melding
E6=Schrijf Smoren Activatie Vlag
F9=Totaal NAND Programering (pagina's)
FB=Totaal NAND Lezen

[SmartCorsair] ;Added 6.2.0
01=Raw Lees Fout Factor
05=End-to-End Data Fouten Gecorrigeerd
09=Bedrijfs Uren
0C=Schijf inschakelen
AA=Reserve Block's
AC=Wis Fouten
AE=Onverwachte Power Onderbrekingen
B5=Programma Fouten
BB=Gerapporteerde Niet Corrigeerbare Fouten
C2=Temperatuur
C4=Heringedeelde Events
E7=SSD Resterende Levensduur
F1=Tijdsduur GB Geschreven
F2=Tijdsduur GB Gelezen

[SmartToshiba] ;Added 6.2.0
01=Lees Fout Factor
02=Data Doorvoersnelheid
03=Opstart Tijd
04=Start/Stop Aantal
05=Heringedeelde Sectoren
07=Zoek Fouten Factor
08=Zoek tijd prestaties
09=Bedrijfs Uren
0A=Herstart's
0B=Herijkingen
0C=Inschakelingen
A7=SSD Bescherming Modus
A8=SATA PHY Fouten
A9=Totaal Slechte Block's
AD=Erase Count
C0=Onverwachte Power Onderbrekingen
C2=Temperatuur
C4=Herverdeeld Events
C5=Huidig Wachtende Sectoren
C6=Niet Corrigeerbare Sectoren
F1=Totaal Host Schrijven
F2=Totaal Host Lezen

[SmartSanDiskGb] ;Added 6.2.0
05=Herverdeelde Block's
09=Bedrijfs Uren
0C=Schijf inschakelen
A6=Min. W/E Cyclus
A7=Max. Slechte Block's/Dood
A8=Maximum Wis Cyclus
A9=Totaal Slechte Block's
AB=Programma Fouten
AC=Wis Fouten
AD=Gemiddeld Wissen Cyclus
AE=Onverwachte  Power Onderbrekingen
BB=Geraporteerde Niet Herstelbare Fouten
C2=Temperatuur
D4=SATA PHY Fouten
E6=Percentage Totaal P/E
E8=Reserve Block's Resterend
E9=Totaal GB Schrijven naar NAND
F1=Totaal GB Schrijven
F2=Totaal GB Lezen

[SmartKingston] ;Added 6.6.0
01=Lees Fout Factor
02=Data Doorvoersnelheid
03=Opstart Tijd
05=Heringedeelde Sectoren
07=Zoek Fouten Aantal
08=Zoek tijd prestaties
09=Bedrijfs Uren
0A=Herstart's
0C=Power Cycle
A8=SATA PHY Fouten
AA=Slechte Block's
AD=Wissen
AF=Slechte Cluster's Tabellen
BB=Niet Corrigeerbare Fouten
C0=Onveilig Afsluiten
C2=Temperatuur
C4=Later Slechte Block's
C5=Huidig Wachtende Sectoren
C7=CRC Fouten
DA=CRC Fouten
E7=SSD Levensduur Over
E9=Tijdsduur Geschreven naar Flash
F0=Schrijf Kop
F1=Host Geschreven
F2=Host Gelezen
F4=Gem. Wissen
F5=Max Wissen
F6=Totaal Wissen

[SmartNVMe] ;Added 6.7.0
01=Kritieke Waarschuwing
02=Composite Temperatuur
03=Beschikbare Reserve's
04=Beschikbare reserve drempel
05=Percentage Gebruikt
06=Data Units Lezen
07=Data Units Schrijven
08=Host Lees Opdrachten
09=Host Schrijf Opdrachten
0A=Beheer Bezet Tijd
0B=Power Cycles
0C=Bedrijfs Uren
0D=Onveilige Afsluiten
0E=Media en Data Integriteit Fouten
0F=Fout Informatie Logboeken

[SmartRealtek] ;Added by Realtek
01=Raw data error rate
05=Reallocated sector count
09=Power on hour count
0C=Power cycle count
A1=GDN
A2=Total erase count
A3=Max PE cycle
A4=Average erase count
A5=Initial bad block count
A6=Total bad block count
A7=SSD protect mode
A8=SATA Phy error count
A9=Health
AB=Program fail count
AC=Erase fail count
AE=Unexpected power loss count
AF=ECC fail count
B5=Unaligned access count
BB=Reported uncorrectable error
C2=Enclosure temperature
C3=Cumulative corrected ecc
C4=Reallocation event count
C7=Ultra DMA CRC error count
CE=Min. erase count
CF=Max erase count
E7=Lifetime left
E8=Available reserved space
F1=Write life time
F2=Read life time
F9=Total GB written to NAND (TLC)
FA=Total GB written to NAND (SLC)

[SmartSKhynix] ; Updated 8.8.0
01=Read Error Rate
05=Re-Assigned Sector Count
09=Power-On Hours
0C=Power Cycle Count
64=Total Erase Count
A8=Min. Erase Count
A9=Max. Erase Count
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
AF=Program Fail Count(Worst Case)
B0=Erase Fail Count(Worst Case)
B1=Wear Leveling Count
B2=Used Reseved Block Count(Worst Case)
B3=Used Reseved Block Count(SSD Total)
B4=UnUsed Reseved Block Count(SSD Total)
B5=Program Fail Count(SSD Total)
B6=Erase Fail Count(SSD Total)
B7=SATA Downshift Count
B8=End-to-End Error Detection Count
BB=Uncorrectable Error Count
BC=Command Timeout Count
BF=Op Shock Event Count
C2=Temperature
C3=ECC Rate
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
C7=CRC Error Count
C9=Uncorrectable Soft Read Error Rate
CC=Soft ECC Correction Rate
D4=Phy Error Count
E7=SSD Life Left
E9=SSD Life Left
EA=NAND Written
F1=Total LBA Written
F2=Total LBA Read
FA=Total Number of NAND Read Retries

[SmartKioxia]
09=Power-On Hours Count
0C=Device Power Cycle Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Bad Block Count
AD=Erase Count (User Data)
C0=Unexpected Power Loss Count
C2=Temperature
F1=Host Writes

[SmartWdc]
01=Read Error Rate
05=Reassigned Block Count
09=Power On Hours
0C=Power Cycle Count
A5=Block Erase Count (SLC)
A6=Minimum P/E Cycles
A7=Maximum Bad Blocks per die
A8=Maximum P/E Cycles
A9=Total Bad Block
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average P/E Cycles
AE=Unexpected Power Loss Count
B8=End-to-End Error Detection/Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
C2=Temperature
C7=CRC Error Count
D4=SATA PHY Error
E6=Media Wearout Indicator
E8=Available Reserve Space
E9=NAND GB Written
EA=NAND GB Written (SLC)
EE=Media Wearout Indicator (Cycles Remaining)
F1=Total GB Written
F2=Total GB Read
F4=Temperature Throttle Status
F9=NAND GB Written

[SmartKingstonSuv]
01=Read Error Rate
05=Reallocated Sector Count
09=Power On Hours
0C=Power Cycle Count
AA=Used Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Off Count
AF=Program Fail Count Worst Die
B0=Erase Fail Count Worst Die
B1=Wear Leveling Count
B2=Used Reserved Block Count worst Die
B4=Unused Reserved Block Count (SSD Total)
BB=Reported Uncorrectable Errors
C2=Temperature
C3=On-the-Fly ECC Error Count
C4=Reallocation Event Count
C5=Pending Sector Count
C7=UDMA CRC Error Count
C9=Uncorrectable Read Error Rate
CC=Soft ECC Correction Rate
E7=SSD Life Left
EA=Lifetime Nand Writes
F1=Lifetime Host Writes
F2=Lifetime Host Reads
FA=Total Number of NAND Read Retries

[SmartKingstonKC600]
01=Read Error Rate
05=Re-Allocated NAND Block Count
09=Power-On Hours
0C=Power Cycle Count
94=Reserved
95=Reserved
96=Reserved
97=SLC Average Erase Count
9F=DRAM 1 bit Error Count
A0=Reported UECC (UnCorrectable) Errors
A1=Available Reserved Space
A4=Reserved
A5=Reserved
A6=Reserved
A7=Average Erase Count
A8=Reserved
A9=Percentage Of Rated Lifetime Remaining
B1=Reserved
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power Loss Count
C2=Device Temperature
C3=Hardware ECC Recovered
C4=Reallocation Event Count
C7=UDMA CRC Error Count
E7=Percentage of Rated Lifetime Remaining
E8=Unused Reserved Block Count
F1=Total LBAs Written
F2=Total LBAs Read
F5=Total Media Writes

[SmartKingstonDC500]
01=Host UNC Error Count
09=Power on Hours
0C=Power On / Off Cycle
A7=Protect mode
A8=SATA PHY Error Count
A9=Bad Block Rate
AA=Bad Block Information
AC=Erase Failure Count
AD=Erase Count
B5=Program Fail Count
B6=Erase Failure Count
BB=Host UNC Error Count
C0=Unexpected Power Loss Count
C2=Temperature
C4=Total Later Bad Block Count
C7=CRC Error Count
CF=Thermal Throttling Count
DA=CRC Error Count
E7=SSD Life Remaining
E8=Read Fail Count
E9=NAND Write
F1=Host Write
F2=Host Read
F4=Avg Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartKingstonSA400]
01=Uncorrectable Errors
09=Power On Hours
0C=Power Cycles
94=Vendor Unique
95=Vendor Unique
A7=Vendor Unique
A8=SATA PHY Error Count
A9=Vendor Unique
AA=Bad Block Count
AC=Vendor Unique
AD=Erase Count
B5=Vendor Unique
B6=Vendor Unique
BB=Uncorrectable ECC Errors
C2=Temperature
C4=Reallocation Events
C7=SATA CRC Error
DA=CRC Error Count
E7=SSD Wear Indicator
E9=Lifetime Nand Writes
F1=Lifetime Writes from Host
F2=Lifetime Read from Host
F4=Average Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartSsstc]
01=Raw Read Error Rate
05=Reallocated Block Count
09=Power On Hours
0C=Power Cycle Count
AA=Available Reserved Space
AB=Program Fail Count(Total)
AC=Erase Fail Count(Total)
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
AF=Program Fail count (Worst case)
B0=Erase Fail Count (Worst case)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst case)
B3=Used Reserved Block Count (Total)
B4=Unused Reserved Block Count (Total)
B7=SATA Interface Down shift
B8=End-to-End Data Errors Count
BB=Uncorrectable Error Count
BC=Command Time out
C2=Drive Temperature
C3=ECC rate
C6=OffLine Uncorrectable Error Count
C7=SATA CRC Error Count
E5=Power Loss Protection Failure
E7=Percentage Lifetime Remaining
E8=Available Reserved Space 
E9=NAND GB Written
F1=Total Host Write
F2=Total Host Read 
F3=NAND GB Written

[SmartIntelDc]
01=Raw Read Error Count
05=Reallocated Flash Block Count
09=Power-On Hours Count
0C=Power Cycle Count
0E=Device Capacity
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Available
AC=Total Block Erase Failure
AD=Per Block Max Erase Count
AE=Unexpected Power Loss Count
AF=Average Erase Count
B0=Power Loss Protection Error
B5=Total Block Program Failure
B8=End-to-End Error Detection Count
BB=Uncorrectable Error Count
C2=Temperature
C5=Pending Sector Count
C6=Offline Uncorrectable Error Count
C7=CRC Error Count
CA=Percentage of Drive Life Used
E2=Timed Workload - Media Wear
E3=Timed Workload - Host Read/Write Ratio
E4=Timed Workload Timer
EA=Total Host Bytes Read
EB=Total Host Bytes/Sectors Written
F1=Total Nand Bytes/Sectors Written

[SmartApacer]
09=Power on Hours
0C=Power Cycle Count
A3=Maximum Erase Count
A4=Average Erase Count
A6=Total Later Bad Block Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
AB=Program Fail Count
AC=Erase Fail Count
AF=Bad Cluster Table Count
C0=Unexpected Power Loss Count
C2=Temperature
E7=Lifetime Left
F1=Total Sectors Write

[SmartSiliconMotion]
01=Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
94=SLC Total Erase Count
95=SLC Maximum Erase Count
96=SLC Minimum Erase Count
97=SLC Average Erase Count
9F=DRAM 1 bit Error Count
A0=Uncorrectable sectors count when read/write
A1=Number of Valid Spare Blocks
A2=Number of Cache Data Block
A3=Number of Initial Invalid Blocks
A4=Total Erase Count
A5=Maximum Erase Count
A6=Minimum Erase Count
A7=Average Erase Count
A8=Max Erase Count of Spec
A9=Remain Life
AF=Program fail count in worst die
B0=Erase fail count in worst die
B1=Total Wear Level Count
B2=Runtime Invalid Block Count
B5=Total Program Fail Count
B6=Total Erase Fail Count
BB=Uncorrectable Error Count
C0=Power-Off Retract Count
C2=Temperature
C3=Hardware ECC Recovered
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Error Count Off-line
C7=Ultra DMA CRC Error Count
E8=Available Reserved Space
F1=Total LBA Written
F2=Total LBA Read
F5=Flash Write Sector Count

[SmartJMicron66x]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase Count
AF=Bad Cluster Table Count
B4=Spare Block Count
C0=Unexpected Power Loss Count
C2=Temperature
C5=Current Pending Sector Count
E7=Drive Life
E9=Write Sector Count (NAND)
F0=Write Head
F1=Total LBA Written
F2=Total LBA Read

[SmartPhison]
01=Read Error Rate
09=Power on Hours
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase Count
C0=Unexpected Power Loss Count
C2=Temperature
DA=Number of CRC Error
E7=SSD Life Left
F1=Host Writes

[SmartSeagate]
01=Read Error Rate
05=Retired Sectors Count
09=Power On Hours
0C=Power Cycle Count
10=Spare Blocks Available
11=Remaining Spare Blocks
A8=SATA PHY Error Count
AA=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power loss Count
C2=Temperature
C9=Soft Error Rate
CC=Soft ECC Correction Rate
DA=CRC Error Count
E7=SSD Life Left
E8=Read Failure Block Count
E9=NAND GiB Written
EA=Lifetime Writes To Flash
EB=NAND sectors Written
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
FA=Lifetime NAND Read Retries

[SmartSeagateIronWolf]
01=Raw Read Error Rate
05=Reallocated Sector Count
09=Power On Hours
0C=Power Cycle Count
64=Flash Gigabytes Erased
66=Lifetime PS4 Entry Count
67=Lifetime PS3 Entry Count
AA=Grown Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Program/Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B7=SATA/PCIe Interface Downshift Count
BB=Uncorrectable ECC Count
C2=Temperature
C3=RAISE ECC Correctable Count
C6=Uncorrectable Read Error Count
C7=SATA R-Error (CRC) Error Count
E6=Drive Life Protection Status
E7=SSD Life Left
E8=Available Reserved Space
E9=Lifetime Writes to Flash
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
F3=Free Space

[SmartMarvell] ; Added 8.8.3
05=Number of New Bad Block
09=Power On Hours
0C=Power Cycle Count
A4=Total Erase Count
A5=Maximum Erase Count
A6=Minimum Erase Count
A7=Average Erase Count
C0=Power off Retract Count
C2=Temperature
C7=SATA CRC Error Count
F1=Total Written
F2=Total Read

[SmartMaxiotek] ; Added 8.8.6
05=Reallocated Sector Count
09=Power-On Hours
0C=Drive Power Cycle Count
A7=SSD Protect Mode
A8=PHY Error Count
A9=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AF=Bad Cluster Table Count
B1=Read Retry Count
B4=Spare Block Count Left
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Temperature
C4=Reallocated Event Count
C7=UDMA CRC Error Count
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=Minimum Erase Count of SLC block
D2=Maximum Erase Count of SLC block
D3=Average Erase Count of SLC block
E7=SSD Life Left
E9=Write Counts Sectors to Nand
EA=Read Counts Sectors from Nand
F1=Write Sector Count
F2=Read Sector Count
F5=Bit Error Count

[SmartSeagateBarraCuda] ; Added 8.9.0
01=UECC Error Count
05=Retired Sectors Count
09=Power On Hours
0C=Power Cycle Count
10=Spare Blocks Available
11=Remaining Spare Blocks
A8=SATA PHY Error Count
AA=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
C0=Unexpected Power loss Count
C2=Temperature
C9=Soft Error Rate
CC=Soft ECC Correction Rate
DA=CRC Error Count
E7=SSD Life Left
E8=Read Failure Block Count
E9=NAND GiB Written
EA=Lifetime Writes To Flash
EB=NAND sectors Written
F1=Lifetime Writes From Host
F2=Lifetime Reads From Host
FA=Lifetime NAND Read Retries

[SmartYmtc] ; Added 8.10.0
05=New Bad Block Count
09=Power-On Hours Count
0C=Power Cycle Count
AA=Max Bad Block Count
A8=SATA PHY Error Count
A9=Bad Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
AF=Bad Cluster Count
B7=SATA Interface Downshift
B8=End to End Error Detection/Correction Count
BB=Uncorrectable Error Count
BE=Temperature
C0=Unexpected Power Loss Count
C4=Re-allocated Event Count
C7=CRC Error Count
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=SLC Minimum Erase Count
D2=SLC Maximum Erase Count
D3=SLC Average Erase Count
E7=SSD Life Left
E9=Write sector count to NAND
EA=Read sector count to NAND
F1=Total LBA written
F2=Total LBA Read
F3=NAND Temperature
F5=Bit Error Count

[SmartScy] ;Added 8.12.8
01=Raw Read Error Rate
05=Reallocated Sector Count
07=Seek Error Rate
09=Power-On Hours
0C=Drive Power Cycle Count
A7=Average Erase Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
B1=Read Retry Count
B4=Spare Block Count Left
B7=Runtime Bad Block
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Controlled Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocated Event Count
C5=Current Pending Sector
C7=UDMA CRC Error Count
E7=SSD Life Left
F1=Total LBAs Written
F2=Total LBAs Read
F5=Total Nand Flash Written

[SmartRecadata] ;Added 8.14.0
07=Seek Error Rate
09=Power-On Hours
0C=Drive Power Cycle Count
A7=Average erase count
AB=Program Fail Count
AC=Erase Fail Count
AD=Erase Count
B1=Read Retry Count
B4=Spare Block Count Left
B7=Runtime Bad Block
BB=Reported UNC Errors
C0=Unexpected Power Loss Count
C2=Controlled temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocated Event Count
C5=Current Pending Sector
C7=UDMA CRC Error Count
E7=SSD Life Left
F1=Total LBAs written
F2=Total LBAs read
F5=Total Nand Flash Written

[SmartSanDiskHp] ;Added 8.17.0
01=Raw Read Error Rate
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Wear Leveling Count
AE=Unexpected Power Loss Count
B0=Unused Reserved Block Count
B7=SATA Interface Downshift Count
B8=End to End Error Detection/Correction Count
BB=Uncorrectable Error Count
BC=Command Time Out
BE=Airflow Temperature
C2=Temperature
C4=Reallocated Event Count
C7=CRC Error Count
C9=SSD Life Left
E6=Media Wearout Indicator
F1=Total LBAs Written
F2=Total LBAs Read
F3=Throttle Statistics
F4=Temperature Throttle Status
F9=TLC NAND GB Writes

[SmartSanDiskHpVenus] ;Added 8.17.0
01=Raw Read Error Rate
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Wear Leveling Count
AE=Unexpected Power Loss Count
B0=Unused Reserved Block Count
B7=SATA Interface Downshift Count
B8=End to End Error Detection/Correction Count
BB=Uncorrectable Error Count
BC=Command Time Out
BE=Airflow Temperature
C2=Temperature
C4=Reallocated Event Count
C7=CRC Error Count
C9=SSD Life Left
E6=Media Wearout Indicator
F1=Total LBAs Written
F2=Total LBAs Read
F3=Total NAND Writes
F4=Temperature Throttle Status
F9=TLC NAND GB Writes

[SmartSanDiskDell] ;Added 8.17.0
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
AF=Program Fail Count (Worst Case Component)
B0=Erase Fail Count (Worst Case Component)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst Case Component)
B3=Used Reserved Block Count (SSD Total)
B4=Remaining Reserved Block Count (SSD Total)
B5=Program Fail Count (SSD Total)
B6=Erase Fail Count (SSD Total)
BB=Uncorrectable Error Count
C2=Temperature
C3=ECC Rate
C7=CRC Error Count
E6=Media Wearout Indicator
EE=Media Wearout Indicator (Cycles Remaining)
F1=Total LBAs Written
F2=Total LBAs Read

[SmartSanDiskLenovo] ;Added 8.17.0
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
A6=Minimum P/E Cycles
A7=Maximum Bad Blocks per Die
A8=Maximum P/E cycles
A9=Total Bad Blocks
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average P/E Cycles Attribute
AE=Unexpected Power Loss Count
B2=Used Reserved Block Count
B4=Remaining Reserved Block Count
B8=End to End Error Detection/Correction Count
BB=UECC Count
BC=Command Time Out
C2=Temperature
C7=SATA CRC Errors
D4=SATA PHY Errors
E6=Media Wearout Indicator
E8=Available Reserved Space
E9=NAND GB Written
EA=NAND GB Written (SLC)
F1=Total Host GB Write
F2=Total GB Read
F3=Throttle Statistics
F4=Thermal Throttle Status

[SmartSanDiskLenovoHelenVenus] ;Added 8.17.0
05=Reassigned Block Count
09=Power On Hours
0C=Drive Power Cycle Count
A6=Minimum P/E Cycles
A7=Maximum Bad Blocks per Die
A8=Maximum P/E cycles
A9=Total Bad Blocks
AA=Grown Bad Blocks
AB=Program Fail Count
AC=Erase Fail Count
AD=Average P/E Cycles Attribute
AE=Unexpected Power Loss Count
B2=Used Reserved Block Count
B4=Remaining Reserved Block Count
B8=End to End Error Detection/Correction Count
BB=UECC Count
BC=Command Time Out
C2=Temperature
C7=SATA CRC Errors
D4=SATA PHY Errors
E8=Available Reserved Space
E9=Media Wearout Indicator
EA=NAND GB Written (SLC)
F1=Total Host GB Write
F2=Total GB Read
F3=Throttle Statistics
F4=Thermal Throttle Status
F9=NAND GB Written (TLC)

[SmartMicronMU03] ;Added 8.17.0
01=Raw Read Error Rate
05=Reallocated NAND Block Count
09=Power On Hours Count
0C=Power Cycle Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Block Erase Count
AE=Unexpected Power Loss Count
B4=Unused Spare NAND Blocks
B5=Non-4K Aligned Access
B7=SATA interface Downshift
B8=Error Correction Count
BB=Reported Uncorrectable Errors
C2=Temperature
C4=Reallocation Event Count
C5=Current Pending ECC Count
C6=SMART Offline Scan Uncorrectable Error Count
C7=UDMA CRC Error Count
CA=Lifetime Remaining
CE=Write Error Rate
D2=Successful RAIN Recovery Count
F0=Host Program Page Count
F1=Total LBAs Written
F2=Total LBAs Read
F3=Total Program Page Count
F6=Cumulative Host Sectors Written
F7=Host Program NAND Pages Count
F8=FTL Program NAND Pages Count

[SmartSanDiskCloud] ;Added 9.0.0
05=Retired Block Count
09=Power On Hours
0D=Count of Uncorrectable ECC Errors
20=Write Amplification multiplied by 100
21=Write Amplification Factor
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Write/Erase Count
AE=Unexpected Power Loss Count
B2=SSD Life Left (upto 0.01%)
BF=Clean Shutdown Count
C0=Unclean Shutdown Count
C2=Temperature
C4=Number of Blocks Reallocated
E6=Percent of Total Write/Erase Count
E8=Spare Blocks Remaining
E9=Total Nand Writes 64GB
EB=Capacitor Health
F1=Total Host Writes 64GB
F2=Total Host Reads 64GB
F4=Lifetime Thermal Throttle Activations
F5=Percent Drive Life Remaining
FD=SPI Tests Remaining
